Extension memory enabled: 
blk1 
blk2 
blk3 
*** VICE Version 2.1 ***
 
Welcome to xvic, the free portable VIC20 Emulator.
 
Current VICE team members:
A. Boose, D. Lem, T. Biczo, A. Dehmel, T. Bretz, A. Matthies,
M. Pottendorfer, M. Brenner, S. Trikaliotis, M. van den Heuvel,
C. Vogelgsang, F. Gennari, M. Kiesel, H. Nuotio, D. Kahlin.
 
This is free software with ABSOLUTELY NO WARRANTY.
See the "About VICE" command for more info.
 
Loading system file `D:\GameBase\DE1FDC~1\EMULAT~1\WINVIC~1.1\VIC20\kernal'.
Loading system file `D:\GameBase\DE1FDC~1\EMULAT~1\WINVIC~1.1\VIC20\basic'.
Loading system file `D:\GameBase\DE1FDC~1\EMULAT~1\WINVIC~1.1\VIC20\chargen'.
VIC20 kernal patched to 901486-07.
LoadLibrary opencbm.dll failed!
MPS-803: Error - Could not load MPS-803 charset 'mps803'.
MPS-803: Error - Cannot load palette file `mps803.vpl'.
NL10: Error - Could not load NL-10 ROM file 'nl10-cbm'.
Loading system file `D:\GameBase\DE1FDC~1\EMULAT~1\WINVIC~1.1\DRIVES\dos1541'.
IECDriveROM: Error - 1541-II ROM image not found.  Hardware-level 1541-II emulation is not available.
IECDriveROM: Error - 1570 ROM image not found.  Hardware-level 1570 emulation is not available.
IECDriveROM: Error - 1571 ROM image not found.  Hardware-level 1571 emulation is not available.
IECDriveROM: Error - 1581 ROM image not found.  Hardware-level 1581 emulation is not available.
IEEEDriveROM: Error - 2031 ROM image not found.  Hardware-level 2031 emulation is not available.
IEEEDriveROM: Error - 2040 ROM image not found.  Hardware-level 2040 emulation is not available.
IEEEDriveROM: Error - 3040 ROM image not found.  Hardware-level 3040 emulation is not available.
IEEEDriveROM: Error - 4040 ROM image not found.  Hardware-level 4040 emulation is not available.
IEEEDriveROM: Error - 1001 ROM image not found.  Hardware-level 1001/8050/8250 emulation is not available.
Drive: Finished loading ROM images.
Refresh rate: 003427D2 / 32.00 = 106814.563
RGB surface...
dwRGBBitCount: 32
dwRBitMask: 00ff0000
dwGBitMask: 0000ff00
dwBBitMask: 000000ff
Sound: Available sound devices: dx wmm dummy fs speed dump wav voc iff aiff ffmpegaudio
Keyboard: Loading keymap `D:\GameBase\DE1FDC~1\EMULAT~1\WINVIC~1.1\VIC20\win_pos.vkm'.
AUTOSTART: Autodetecting image type of `d:\gbgame\0\ubermode.d64'.
Filesystem Image Probe: D64 disk image recognised: d:\gbgame\0\ubermode.d64, 35 tracks.
DriveImage: Unit 8: D64 disk image attached: d:\gbgame\0\ubermode.d64.
VDrive: Unit 8: D64 disk image attached: d:\gbgame\0\ubermode.d64.
AUTOSTART: Attached file `d:\gbgame\0\ubermode.d64' as a disk image.
AUTOSTART: Resetting the machine to autostart 'BOOT'
AUTOSTART: `d:\gbgame\0\ubermode.d64' recognized as disk image.
Main CPU: starting at ($FFFC).
Main CPU: RESET.
Sound: Opened device `dx', speed 22050Hz, fragment size 23ms, buffer size 371ms
RS232DEV: Error - Attempt to close non-open fd 0.
RS232DEV: Error - Attempt to close non-open fd 1.
RS232DEV: Error - Attempt to close non-open fd 2.
RS232DEV: Error - Attempt to close non-open fd 3.
AUTOSTART: Loading program 'BOOT'
AUTOSTART: Starting program.
Writing configuration file `D:\GameBase\DE1FDC~1\EMULAT~1\WINVIC~1.1\vice.ini'.

Exiting...
fdc: Unit 8: D64 disk image detached: d:\gbgame\0\ubermode.d64.
DriveImage: Unit 8: D64 disk image detached: d:\gbgame\0\ubermode.d64.
VDrive: Unit 8: D64 disk image detached: d:\gbgame\0\ubermode.d64.
Sound: Closing device `dx'
